{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":130,"n_cols":5,"rows_kept":130,"merged":[[0,0,0,4],[1,0,1,4],[11,0,11,4],[17,0,17,4],[18,0,18,4],[31,0,31,4],[38,0,38,4],[39,0,39,4],[47,0,47,4],[53,0,53,4],[54,0,54,4],[63,0,63,4],[68,0,68,4],[69,0,69,4],[77,0,77,4],[79,4,80,4],[81,4,82,4],[84,0,84,4],[85,0,85,4],[87,4,90,4],[91,0,91,4],[92,0,92,4],[94,4,95,4],[96,0,96,4],[97,0,97,4],[99,4,102,4],[103,0,103,4],[104,0,104,4],[106,4,109,4],[110,0,110,4],[111,0,111,4],[112,4,115,4],[119,0,119,4],[120,0,120,4],[123,0,123,4],[124,0,124,4],[126,0,126,4],[127,0,127,4],[128,0,128,4],[129,1,129,4]]}
["一、仪表类开关阀"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"执行机构维修包（弹簧薄膜执行机构）","所有规格","每种规格备一台套","包括：膜片、推杆密封O型圈等"]
[2,"执行机构维修包（活塞式执行机构）","所有规格","每种规格备一台套","包括：活塞密封O型圈、四氟导向带、推杆（转轴）密封O型圈等"]
[3,"阀体维修包（直行程）","所有规格","每种规格备一台套","包括：填料、上盖垫片、平衡密封环（如果有必配）、阀座垫片等。"]
[4,"阀体维修包（角行程）","所有规格","每种规格备一台套","包括：填料、中法兰垫片、阀座垫片（石墨、O型圈）、碟簧（如果有必配）、蝶阀密封环（如有必配）、平面轴承、轴瓦等。"]
[5,"电磁阀","所有规格","每种规格备一台套"]
[6,"阀位回讯","所有规格","每种规格备一台套"]
[7,"过滤减压阀（含压力表）","所有规格","每种规格备一台套"]
[8,"气控阀","所有规格","每种规格备一台套"]
["两年备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"阀芯","所有规格","每种规格备一台套"]
[2,"阀座","所有规格","每种规格备一台套"]
[3,"阀杆","所有规格","每种规格备一台套"]
[]
["二、仪表类调节阀"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"执行机构维修包（弹簧薄膜执行机构）","所有规格","每种规格备一台套","包括：膜片、推杆密封O型圈等"]
[null,"执行机构维修包（活塞式执行机构）","所有规格","每种规格备一台套","包括：活塞密封O型圈、四氟导向带、推杆（转轴）密封O型圈等"]
[2,"阀体维修包（直行程）","所有规格","每种规格备一台套","包括：填料、上盖垫片、平衡密封环（如果有必配）、阀座垫片等。"]
[2,"阀体维修包（角行程）","所有规格","每种规格备一台套","包括：填料、中法兰垫片、阀座垫片（石墨、O型圈）、碟簧（如果有必配）、蝶阀密封环（如有必配）、平面轴承、轴瓦等。"]
[3,"定位器","所有规格","每种规格备两台套"]
[4,"压力表","所有规格","每种规格备两台套"]
[5,"O型环","所有规格","每种规格备两台套"]
[6,"过滤减压阀","所有规格","每种规格备两台套"]
[null,"电磁阀（如有）","所有规格","每种规格备一台套"]
[null,"气控阀（如有）","所有规格","每种规格备一台套"]
["3. ","执行机构密封包","所有规格","每种规格备一台套"]
["两年备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"执行机构膜片","所有规格","每种规格备一台套"]
[2,"阀座","所有规格","每种规格备一台套"]
[3,"阀杆","所有规格","每种规格备一台套"]
[4,"阀笼","所有规格","每种规格备一台套"]
[5,"阀芯","所有规格","每种规格备一台套"]
["三、电动执行机构"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"电源板","所有规格","每种规格备一台套"]
[2,"控制板","所有规格","每种规格备一台套"]
[3,"显示器面板","所有规格","每种规格备一台套"]
[4,"力矩传感器","所有规格","每种规格备一台套"]
[5,"遥控器","所有规格","按执行器数量10：1配，不足10台配1只"]
[]
["两年备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"绝对编码器","所有规格","每种规格备一台套"]
[2,"蜗轮蜗杆传动伞齿轮","所有规格","每种规格备一台套"]
[3,"线圈绕组定子、转子","所有规格","每种规格备一台套"]
[4,"手自动离合器","所有规格","每种规格备一台套"]
["四、色谱分析仪"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"色谱仪保险丝","所有规格","一包（20个）"]
[2,"色谱采样阀","所有规格","每种规格备一台套"]
[3,"预处理减压阀","所有规格","每种规格备一台套"]
[4,"快速回路过滤器","所有规格","每种规格备一台套"]
[null,"标液","所有规格","每种规格备一瓶(10L)"]
[null,"载气","所有规格","每种规格备一瓶（40L)"]
[]
["两年备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"FID检测器","所有规格","每种规格备一台套"]
[2,"色谱柱","所有规格","每种规格备一台套"]
[]
["五、在线烟气分析仪"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"信号转换模块","所有规格","每种规格备一台套"]
[2,"快插接头","所有规格","每种规格备一台套"]
[3,"陶瓷滤芯","所有规格","每种规格备一台套"]
[4,"温度传感器","所有规格","每种规格备一台套"]
[null,"氟管","所有规格","每种规格备一台套"]
[null,"螺钉备件","所有规格","每种规格备一台套"]
["两年备件清单"]
["序号","备件名称","单位","同种规格数量","备注"]
[1,"陶瓷滤芯","所有规格","每种规格备一台套"]
[2,"温度传感器","所有规格","每种规格备一台套"]
[3,"石墨垫片","所有规格","每种规格备一台套"]
[4,"温度控制器","所有规格","每种规格备一台套"]
[5,"卡套接头","所有规格","每种规格备一台套"]
["六、温度仪表"]
["开车备件清单"]
["序号","名称","规格参数","数量","备注"]
[1,"双金属温度计含套管","所有规格","每种规格备一台套","同种规格数量大于10个备2套"]
[2,"温度变送器（一体式）含套管","所有规格","每种规格备一台套"]
[3,"温度变送器（分体式）","所有规格","每种规格备一台套"]
[4,"温度传感器含套管（分体式）","所有规格","每种规格备一台套"]
["七、压力仪表"]
["开车备件清单"]
["序号","备件名称","单位","同种规格数量","备注"]
[1,"压力表","所有规格","每种规格备一台套","同种规格数量大于10个备2套"]
[2,"压力/差压变送器（含单、双法兰）","所有规格","每种规格备一台套"]
["八、液位仪表"]
["开车备件清单"]
["序号","备件名称","单位","同种规格数量","备注"]
[1,"浮球/音叉开关","所有规格","每种规格备一台套","同种规格数量大于10个备2套"]
[2,"雷达液位变送器","所有规格","每种规格备一台套"]
[2,"浮筒液位计表头","所有规格","每种规格备一台套"]
[2,"磁致伸缩液位计","所有规格","每种规格备一台套"]
["九、流量仪表"]
["开车备件清单"]
["序号","备件名称","单位","同种规格数量","备注"]
[1,"转子流量计/开关","所有规格","每种规格备一台套","同种规格数量大于10个备2套"]
[2,"质量流量计变送器单元","所有规格","每种规格备一台套"]
[3,"电磁流量计变送器单元","所有规格","每种规格备一台套"]
[4,"涡街流量计变送器单元","所有规格","每种规格备一台套"]
["十、分析仪表"]
["开车备件清单"]
[1,"电导变送器及传感器","所有规格","每种规格备一台套","同种规格数量大于10个备2套"]
[2,"PH变送器及传感器","所有规格","每种规格备一台套"]
[3,"露点分析仪","所有规格","每种规格备一台套"]
[4,"溶氧分析仪","所有规格","每种规格备一台套"]
[5,"在线氧分析仪","所有规格","每种规格备一台套","分析仪整台备件1台，预处理系统配件每种规格备1个"]
[6,"VOCs分析仪","所有规格","每种规格备一台套"]
[1,"有毒可燃气体探测器","所有规格","每种规格备一台套","同种规格数量大于10个备2台"]
["十一、称重仪表"]
["开车备件清单"]
[1,"称重传感器","所有规格","每种规格备一台套"]
[2,"称重仪","所有规格","每种规格备一台套"]
["十二、同位素仪表"]
["开车备件清单"]
[1,"射源液位传感器/变送器","台",1,"每种规格备1PC"]
["十三、DCS、SIS、GDS系统"]
["控制系统的所有硬件（包括但不限于CPU模块、各类I/O模块、通讯模块、系统电源模块、24VDC电源模块及电源冗余模块、安全栅、继电器等）均需提供备件，每种类型的硬件备用数量不应少于10%，且每种至少备1件。"]
["其他仪表（包括未列出来的就地、远传仪表等）"]
[1,"每种规格的仪表至少提供1套备件。"]